POCKETSPHINX_CONTINUOUS(1)

NAME
pocketsphinx_continuous - Run speech recognition in continuous listening mode

SYNOPSIS
pocketsphinx_continuous -hmm hmmdir -dict dictfile [ options ]...

DESCRIPTION

This program opens the audio device and waits for speech. When it detects an utterance, it performs speech recognition on it.

-adcdev
    name for audio input (platform-specific)

-adchdr
    Size of audio file header in bytes (headers are ignored)

-adcin
    Input is raw audio data

-agc
    Automatic gain control for c0 ('max', 'emax', 'noise', or 'none')

-agcthresh
    Initial threshold for automatic gain control

-allphone
    Do phoneme recognition

-alpha
    Preemphasis parameter

-backtrace
    Print back trace of recognition results

-beam
    Beam width applied to every frame in Viterbi search (smaller values mean wider beam)

-bestpath
    Run bestpath (Dijkstra) search over word lattice (3rd pass)

-bestpathlw
    Language model probability weight for bestpath search

-cachesen
    Cache senone scores from first pass search

-cep2spec
    Input is cepstral files, output is log spectral files

-cepdir
    files directory (prefixed to filespecs in control file)

-cepext
    Input files extension (prefixed to filespecs in control file)

-ceplen
    Number of components in the input feature vector

-cmn
    Cepstral mean normalization scheme ('current', 'prior', or 'none')

-cmninit
    Initial values (comma-separated) for cepstral mean when 'prior' is used

-compallsen
    Compute all senone scores in every frame (can be faster when there are many senones)

-ctl
    file listing utterances to be processed

-ctlcount
    No. of utterances to be processed (after skipping -ctloffset entries)

-ctlincr
    Do every Nth line in the control file

-ctloffset
    No. of utterances at the beginning of -ctl file to be skipped

-dict
    pronunciation dictionary (lexicon) input file

-dither
    Add 1/2-bit noise

-doublebw
    Use double bandwidth filters (same center freq)

-dsratio
    Frame GMM computation downsampling ratio

-fbtype
    FB Type of mel_scale or log_linear

-fdict
    word pronunciation dictionary input file

-feat
    Feature stream type, depends on the acoustic model

-fillpen
    Filler word transition penalty

-frate
    Frame rate

-fsg
    state grammar

-fsgbfs
    Force backtrace from FSG final state

-fsgctlfn
    finite state grammar control file

-fsgusealtpron
    Use alternative pronunciations for FSG

-fsgusefiller
    (FSG Mode (Mode 2) only) Insert filler words at each state.

-fwd3g
    Use trigrams in first pass search

-fwdflat
    Run forward flat-lexicon search over word lattice (2nd pass)

-fwdflatbeam
    Beam width applied to every frame in second-pass flat search

-fwdflatefwid
    Minimum number of end frames for a word to be searched in fwdflat search

-fwdflatlw
    Language model probability weight for flat lexicon (2nd pass) decoding

-fwdflatsfwin
    Window of frames in lattice to search for successor words in fwdflat search

-fwdflatwbeam
    Beam width applied to word exits in second-pass flat search

-fwdtree
    Run forward lexicon-tree search (1st pass)

-hmm
    containing acoustic model files.

-hyp
    output file name

-hypseg
    output with segmentation file name

-input_endian
    Endianness of input data, big or little, ignored if NIST or MS Wav

-kdmaxbbi
    Maximum number of Gaussians per leaf node in kd-Trees

-kdmaxdepth
    Maximum depth of kd-Trees to use

-kdtree
    file for Gaussian selection

-latsize
    Lattice size

-lifter
    Length of sin-curve for liftering, or 0 for no liftering.

-live
    Get input from audio hardware

-lm trigram language model input file

-lmctl
    a set of language model

The -hmm and -dict arguments are always required. Either -lm or -fsg is required, depending on whether you are using a statistical language model or a finite-state grammar.

AUTHOR
Written by numerous people at CMU from 1994 onwards. This manual page by David Huggins-Daines <dhuggins@cs.cmu.edu>

COPYRIGHT
Copyright © 1994-2007 Carnegie Mellon University. See the file COPYING included with this package for more information.

SEE ALSO
pocketsphinx_batch(1), sphinx_fe(1).